,Type Comments##OTHER##,Product Family##OTHER##,Model##OTHER##,Material##OTHER##,Manufacturer##OTHER##,Description##OTHER##,Connector Description##OTHER##,Code VVS DNK##OTHER##,Code RSK SWE##OTHER##,Code NRF NOR##OTHER##,Code LVI FIN##OTHER##,Code EAN##OTHER##,Article Number##OTHER##,Nominal Flow##PIPING_FLOW##LITERS_PER_SECOND,Pressure Drop##PIPING_PRESSURE##KILOPASCALS
"G3/8, Chrome","G3/8, Chrome",Mora INXX II,274001,Metal - Mora Armatur - Chrome,Mora Armatur,"INXX II soft, basin mixer (S)",G3/8,-,8276500,-,-,7391887274350,274001,"0,08",300
"G3/8, Matt Black","G3/8, Matt Black",Mora INXX II,274001.12,Metal - Mora Armatur - Matte Black,Mora Armatur,"INXX II soft, basin mixer (S)",G3/8,-,8276501,-,-,7391887274367,274001.12,"0,08",300
"G3/8, Polished Brass","G3/8, Polished Brass",Mora INXX II,274001.60,Metal - Mora Armatur - Polished Brass,Mora Armatur,"INXX II soft, basin mixer (S)",G3/8,-,8276502,-,-,7391887274374,274001.60,"0,08",300
"G3/8, Brushed Brass","G3/8, Brushed Brass",Mora INXX II,274001.62,Metal - Mora Armatur - Brushed Brass,Mora Armatur,"INXX II soft, basin mixer (S)",G3/8,-,8276503,-,-,7391887274381,274001.62,"0,08",300
"G3/8, Chrome, LEED/BREEAM compliant 1","G3/8, Chrome, LEED/BREEAM compliant 1",Mora INXX II,274001.LD1,Metal - Mora Armatur - Chrome,Mora Armatur,"INXX II soft, basin mixer (S), LEED/BREEAM compliant, Flow 3 bar 1.5 l/m",G3/8,-,8276524,-,-,7391887274688,274001.LD1,"0,03",300
"G3/8, Matt Black, LEED/BREEAM compliant 1","G3/8, Matt Black, LEED/BREEAM compliant 1",Mora INXX II,274001.12LD1,Metal - Mora Armatur - Matte Black,Mora Armatur,"INXX II soft, basin mixer (S), LEED/BREEAM compliant, Flow 3 bar 1.5 l/m",G3/8,-,8276525,-,-,7391887274701,274001.12LD1,"0,03",300
"G3/8, Polished Brass, LEED/BREEAM compliant 1","G3/8, Polished Brass, LEED/BREEAM compliant 1",Mora INXX II,274001.60LD1,Metal - Mora Armatur - Polished Brass,Mora Armatur,"INXX II soft, basin mixer (S), LEED/BREEAM compliant, Flow 3 bar 1.5 l/m",G3/8,-,8276528,-,-,7391887274725,274001.60LD1,"0,03",300
"G3/8, Brushed Brass, LEED/BREEAM compliant 1","G3/8, Brushed Brass, LEED/BREEAM compliant 1",Mora INXX II,274001.62LD1,Metal - Mora Armatur - Brushed Brass,Mora Armatur,"INXX II soft, basin mixer (S), LEED/BREEAM compliant, Flow 3 bar 1.5 l/m",G3/8,-,8276529,-,-,7391887274749,274001.62LD1,"0,03",300
"G3/8, Chrome, LEED/BREEAM compliant 3","G3/8, Chrome, LEED/BREEAM compliant 3",Mora INXX II,274001.LD3,Metal - Mora Armatur - Chrome,Mora Armatur,"INXX II soft, basin mixer (S), LEED/BREEAM compliant, Flow 3 bar 3.0 l/m",G3/8,-,8276527,-,-,7391887274695,274001.LD3,"0,05",300
"G3/8, Matt Black, LEED/BREEAM compliant 3","G3/8, Matt Black, LEED/BREEAM compliant 3",Mora INXX II,274001.12LD3,Metal - Mora Armatur - Matte Black,Mora Armatur,"INXX II soft, basin mixer (S), LEED/BREEAM compliant, Flow 3 bar 3.0 l/m",G3/8,-,8276526,-,-,7391887274718,274001.12LD3,"0,05",300
"G3/8, Polished Brass, LEED/BREEAM compliant 3","G3/8, Polished Brass, LEED/BREEAM compliant 3",Mora INXX II,274001.60LD3,Metal - Mora Armatur - Polished Brass,Mora Armatur,"INXX II soft, basin mixer (S), LEED/BREEAM compliant, Flow 3 bar 3.0 l/m",G3/8,-,8276530,-,-,7391887274732,274001.60LD3,"0,05",300
"G3/8, Brushed Brass, LEED/BREEAM compliant 3","G3/8, Brushed Brass, LEED/BREEAM compliant 3",Mora INXX II,274001.62LD3,Metal - Mora Armatur - Brushed Brass,Mora Armatur,"INXX II soft, basin mixer (S), LEED/BREEAM compliant, Flow 3 bar 3.0 l/m",G3/8,-,8276531,-,-,7391887274756,274001.62LD3,"0,05",300
