,Type Comments##OTHER##,Product Family##OTHER##,Model##OTHER##,Material##OTHER##,Manufacturer##OTHER##,Description##OTHER##,Connector Description##OTHER##,Code VVS DNK##OTHER##,Code RSK SWE##OTHER##,Code NRF NOR##OTHER##,Code LVI FIN##OTHER##,Code EAN##OTHER##,Article Number##OTHER##,Nominal Flow##PIPING_FLOW##LITERS_PER_SECOND,Pressure Drop##PIPING_PRESSURE##KILOPASCALS
"G3/8, Chrome","G3/8, Chrome",Mora INXX II,274003,Metal - Mora Armatur - Chrome,Mora Armatur,"INXX II sharp, basin mixer (S)",G3/8,-,8276504,-,-,7391887274398,274003,"0,08",300
"G3/8, Matt Black","G3/8, Matt Black",Mora INXX II,274003.12,Metal - Mora Armatur - Matte Black,Mora Armatur,"INXX II sharp, basin mixer (S)",G3/8,-,8276505,-,-,7391887274404,274003.12,"0,08",300
"G3/8, Polished Brass","G3/8, Polished Brass",Mora INXX II,274003.60,Metal - Mora Armatur - Polished Brass,Mora Armatur,"INXX II sharp, basin mixer (S)",G3/8,-,8276506,-,-,7391887274411,274003.60,"0,08",300
"G3/8, Brushed Brass","G3/8, Brushed Brass",Mora INXX II,274003.62,Metal - Mora Armatur - Brushed Brass,Mora Armatur,"INXX II sharp, basin mixer (S)",G3/8,-,8276507,-,-,7391887274428,274003.62,"0,08",300
"G3/8, Chrome, LEED/BREEAM compliant 1","G3/8, Chrome, LEED/BREEAM compliant 1",Mora INXX II,274003.LD1,Metal - Mora Armatur - Chrome,Mora Armatur,"INXX II sharp, basin mixer (S), LEED/BREEAM compliant, Flow 3 bar 1.5 l/m",G3/8,-,8276532,-,-,7391887274763,274003.LD1,"0,03",300
"G3/8, Matt Black, LEED/BREEAM compliant 1","G3/8, Matt Black, LEED/BREEAM compliant 1",Mora INXX II,274003.12LD1,Metal - Mora Armatur - Matte Black,Mora Armatur,"INXX II sharp, basin mixer (S), LEED/BREEAM compliant, Flow 3 bar 1.5 l/m",G3/8,-,8276533,-,-,7391887274787,274003.12LD1,"0,03",300
"G3/8, Polished Brass, LEED/BREEAM compliant 1","G3/8, Polished Brass, LEED/BREEAM compliant 1",Mora INXX II,274003.60LD1,Metal - Mora Armatur - Polished Brass,Mora Armatur,"INXX II sharp, basin mixer (S), LEED/BREEAM compliant, Flow 3 bar 1.5 l/m",G3/8,-,8276534,-,-,7391887274800,274003.60LD1,"0,03",300
"G3/8, Brushed Brass, LEED/BREEAM compliant 1","G3/8, Brushed Brass, LEED/BREEAM compliant 1",Mora INXX II,274003.62LD1,Metal - Mora Armatur - Brushed Brass,Mora Armatur,"INXX II sharp, basin mixer (S), LEED/BREEAM compliant, Flow 3 bar 1.5 l/m",G3/8,-,8276539,-,-,7391887274824,274003.62LD1,"0,03",300
"G3/8, Chrome, LEED/BREEAM compliant 3","G3/8, Chrome, LEED/BREEAM compliant 3",Mora INXX II,274003.LD3,Metal - Mora Armatur - Chrome,Mora Armatur,"INXX II sharp, basin mixer (S), LEED/BREEAM compliant, Flow 3 bar 3.0 l/m",G3/8,-,8276536,-,-,7391887274770,274003.LD3,"0,05",300
"G3/8, Matt Black, LEED/BREEAM compliant 3","G3/8, Matt Black, LEED/BREEAM compliant 3",Mora INXX II,274003.12LD3,Metal - Mora Armatur - Matte Black,Mora Armatur,"INXX II sharp, basin mixer (S), LEED/BREEAM compliant, Flow 3 bar 3.0 l/m",G3/8,-,8276537,-,-,7391887274794,274003.12LD3,"0,05",300
"G3/8, Polished Brass, LEED/BREEAM compliant 3","G3/8, Polished Brass, LEED/BREEAM compliant 3",Mora INXX II,274003.60LD3,Metal - Mora Armatur - Polished Brass,Mora Armatur,"INXX II sharp, basin mixer (S), LEED/BREEAM compliant, Flow 3 bar 3.0 l/m",G3/8,-,8276538,-,-,7391887274817,274003.60LD3,"0,05",300
"G3/8, Brushed Brass, LEED/BREEAM compliant 3","G3/8, Brushed Brass, LEED/BREEAM compliant 3",Mora INXX II,274003.62LD3,Metal - Mora Armatur - Brushed Brass,Mora Armatur,"INXX II sharp, basin mixer (S), LEED/BREEAM compliant, Flow 3 bar 3.0 l/m",G3/8,-,8276539,-,-,7391887274831,274003.62LD3,"0,05",300